Installation Guide for   
Horizon Peripherals Intelligence

August 2020

Table of Contents

[Overview 1](#_Toc48136371)

[System Requirement 1](#_Toc48136372)

[Downloadable Components 2](#_Toc48136373)

[Web OVA Deployment Guide 2](#_Toc48136374)

[How to Install 2](#_Toc48136375)

[After the Installation 5](#_Toc48136376)

[HorizonPeripheralsAgent Install Guide 6](#_Toc48136377)

[Installation 6](#_Toc48136378)

[After the Installation 9](#_Toc48136379)

[HorizonPeripheralsClient Install Guide 10](#_Toc48136380)

[Uninstall 11](#_Toc48136381)

[Change HTTPS Security Certificate Settings (Optional) 12](#_Toc48136382)

# Overview

This is the overall installation guide for Horizon Peripherals Intelligence.

## System Requirement

We only support Horizon Windows client and Windows agent for device diagnosis in the current scope.

The HorizonPeripheralsAgent and HorizonPeripheralsClient installers can be installed on below Windows OS that is compatible with VMware Horizon 7 and later -

Client OS - Windows 7, Windows 10

Agent OS -Windows 7, Windows 10, Windows server 2012R2, 2016, 2019

The web OVA is built on VMware Photon OS 3.0 which is compatible with ESXi 6.5 and later

## Downloadable Components

There are three downloadable components in this project.

1. Web OVA template – device intelligence diagnosis web service host.
2. HorizonPeripheralsAgent installer – A light-weighted diagnosis agent with simplified UI for end user to start a diagnosis for peripheral devices. Installed on the Horizon Windows agent machine.
3. HorizonPeripheralsClient installer – A light-weighted diagnosis plugin to be installed on Horizon Windows client machine

Generally, there are two ways to deploy the services and components in your Horizon environment.


1. Skip the web OVA deployment part if you are inside VMware corporation network.   
   We have set up a local web service (djintelligence.eng.vmware.com) for VMware internal users. So if you are inside VMware corporate network, you can skip the web OVA deployment part. It is sufficient to only install the HorizonPeripheralsAgent and HorizonPeripheralsClient. Follow the installation guides starting from HorizonPeripheralsAgent Install Guide.
2. Setup all of the three components if you are outside VMware corporation network.  
   If you are external customer and users, you need to setup the web OVA server and install the HorizonPeripheralsClient and HorizonPeripheralsAgent programs in your local environment following the guides below.

# Web OVA Deployment Guide


## How to Install

Download the web OVA file to your local machine. The OVA file is compatible with vSphere 6.5 and later version. Follow the general workflow to deploy the OVA template. You can refer to [vSphere guide](https://docs.vmware.com/en/VMware-vSphere/6.5/com.vmware.vsphere.vm_admin.doc/GUID-17BEDA21-43F6-41F4-8FB2-E01D275FE9B4.html). Please pay special attention to below steps and values.


In the Select storage page, choose a valid datastore and Thin Provision for virtual disk format.



In the Select Network, choose a valid virtual network name in your setup (In this example, it is VM Network). Choose Static-Manual as the IP allocation settings.



In the Customize template, there are 6 optional settings provided.

Hostname**:**

If not configured, the default name djintelligence.eng.vmware.com will be used. We suggest set the hostname to a DNS resolvable name in your network environment.

IP Address/Netmask/Gateway:

If any of these 3 settings are not configured, the default DHCP network profile will be used for the OVA deployment. Namely, you should either configure the three settings all together to set a static network profile or leave all of them empty to utilize the DHCP service in your network.

DNS Domain:Optional**.**


DNS Server: Optional.

Notice:

1. Only IPv4 network is supported.
2. We don’t provide complete format and compatibility checks for these settings. Please pay attention to your inputs while configurating these settings carefully. For instance, wrong format of the IP address will result in invalid IP network after importing the OVA which makes the web service unavailable after OVA deployment.
3. After the OVA is imported, power it on. The above customized network settings will be applied automatically in minutes. The web service will be auto-started as well.

## After the Installation

Open the <https://<webova_servername>:8090> , with your configured hostname of the web OVA server.


****

In the home page, users could download the HorizonPeripheralsAgent and HorizonPeripheralsClient installers. This is a convenient way for Horizon admin to distribute the HorizonPeripheralsClient and HorizonPeripheralsAgent installers to end users instead of asking them to download from the VMware Fling web site.

# HorizonPeripheralsAgent Install Guide

## Installation


HorizonPeripheralsAgent.msi is the installer to be run on your Horizon agent machine. The web server address and port number need to be configured to the correct value firstly. If you don’t know the value, you can use the default one and change it after the installation by editing the config file.



There are 2 options in the following installer setup page – Custom and Complete Installations. To make full use of the installer capabilities, we suggest Complete installation with admin privilege.


1. If you launch the installer with admin privilege, choose Complete option. The feature selection page will be skipped. Both features (filecopy and autolaunch) will be installed together. Change the installation directory if you want. By default, it is C:\HorizonPeripheralsAgent\ directory.

The HorizonPeripheralsAgent.exe will be auto launched after horizon client connects to a new remote desktop or app session.



1. If you launch the installer with normal user privilege, choose the Custom option. There are two features in the custom setup page – Filecopy and Autolaunch. The Autolaunch feature is deselected by default. You can change the installation directory. By default, it is C:\HorizonPeripheralsAgent\ directory.


You need to manually click the HorizonPeripheralsAgent.exe under installation directory to launch it after successful installation.



* Filecopy feature will copy all necessary files to the installation directory you choose.
* Autolaunch feature will add registry entries in HKLM path. These registries make HorizonPeripheralsAgent.exe launch automatically whenever you freshly login a Horizon desktop or app session. The registries are –


***“HKLM\\Software\\VMware, Inc.\\VMware VDM\\UnityShell\\Run****”*

***“HKLM\SOFTWARE\Microsoft\Windows\CurrentVersion\Run*”**



After the Installation


The hpagentconfig.ini under the installation folder contains the web server address and port which are configured during installation. If you don’t input them correctly during installation, you could manually change them by editing this config file.



# HorizonPeripheralsClient Install Guide


HorizonPeripheralsClient.msi is the installer to be run on your Horizon client machine. It doesn’t require the administrator privilege to run.

You can choose the installation directory for HorizonPeripheralsClient. By default, it is C:\HorizonPeripheralsClient.



# Uninstall

Go to the Uninstall a program entry in Control Panel. Uninstall the HorizonPeripheralsClient and HorizonPeripheralsAgent programs.



# Change HTTPS Security Certificate Settings (Optional)

By default, a valid certificate will be generated with the web OVA server’s FQDN signed by a VMware internal rootCA after the deployment of Web OVA. This cert is then used by the HTTPS communication between HorizonPeripheralsAgent and web OVA server.

If you want to replace the auto-generated cert with another valid cert singed by another well-known rootCA instead of the VMware rootCA, please follow the steps below manually.

1. Apply for a valid cert from a well-known rootCA. Get the private key (<fqdn>.key) and cert file (<fqdn>.crt) ready.
2. On web OVAOVA server, copy the key and cert files to /etc/nginx/ folder. Edit the /etc/nginx/nginx.conf to replace the ssl\_certificate and ssl\_certificate\_key options with <fqdn>.crt and <fqdn>.key. Reboot the web OVA server to apply the change.
3. Get the public certificate of the well-known rootCA (rootca.pem). Copy it to the HorizonPeripheralsAgent install directory on Horizon agent machine.
4. Relaunch HorizonPeripheralsAgent.exe to apply the change.